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Enter the information provided by your Internet Service Provider (ISP).

DNS AND ADVANCED SETTINGS

DNS setting are automaticlly configured when your connection is estabablished with the I5p.
ISP DNS server setting can be overriden by entering in the DNS IP address below. However,
dvanced: Web Filtering will override all setting made here, as well as the ones provided during
connection.
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